iCarsoft ProfessionalMulti-system Auto DiagnosticToolVAWS V2.0 for Audi/VW/Seat/Skoda, the Update version of VAG II.

iCarsoft VAWS V2.0 is a Professional and powerful vehicle fault diagnosis tool developed by iCarsoft Technology Inc. With a 4.0” TFT LCD and unique diagnostic software, it features full ECU diagnosis of single vehicle brand and test modes mainly include: CANBUS, ISO9141, KWP2000, and J1850etc.Itenables technicians to accurately diagnose complex problems.

Based on VAG II, more functions are added to VAWS V2.0:
BMS reset
Battery Voltage Test
Data Print

Notice:
iCarsoft VAWS V2.0 scanners just work on Audi/VW/Seat/Skoda with OBD II protocol,
if your vehicle were produced before year2005 or after year 2017, please kindly confirm with us about the compatibility before purchasing !
If you want to test some specific functions, please also kindly confirm with us before purchasing, thank you !

Product Features:
1. iCarsoft VAWS V2.0 can do it all-reads and clears trouble codes on most of the systems such as engine, transmission, ABS and airbag etc.
2. Applies to the single Brand of most models of Audi/VW/Seat/Skoda which equipped with OBDII-16 DLC
3. Support OBDII/EOBD Ten Modes of Operation
4. Full System Diagnosis
5. Read &Clear DTC
6. Read Live Data 
7. Support special functions: Oil Service Reset, EPB Reset, DPF reset, SAS Reset, ETCs reset and BMS Reset and Injector Programming
8. Support Data Review
9. The Print Data function allows you printing out diagnostic data recorded by the scan tool or customized test reports.
10. Battery test allows you getting the voltage of battery with OBD port by the scan tool when the engine starts.
11. DTC Library to lookup when user is operating this tool.
12. Easy To Use With Silicone Keys
13. Full Speed Upgrade Via USB2.0
14. 4.0″TFT LCD, 480*320 Pixels
15. Multi-language: English, German, Dutch, Spanish, French.

Special functions:
*** Varies across year and model ***
Oil Service Reset Function
The VAWS V2.0 allow you to reset OilService in a click of a button on supported vehicles. On vehicles where a manual reset is required, the tool will guide you through the full process step-by-step.

 EPB Reset Function:
This electric parking brake (EPB) function has a multitude of uses to maintain the electronic braking systemssafelyandeffectively. 
The applications include deactivating/activating the brake control system, assisting with brake fluid control, brake diagnostics, opening and closing brake pads, setting brakes after disc or pad replacement and also reading and clearing EPB/SBC trouble codes. It is also capable of retrieving Fault Codes information from the ECU.
DPF Regeneration or Replacement
Carry out a forced Diesel Particulate Filter (DPF) Regeneration on supported vehicles - this MUST be done by trained personnel. Required when the DPF filter blockage reaches levels where passive or active regeneration is unable to burn off the excess soot. 
SAS Reset Function
The Steering Angle Sensor (SAS) is used to measure the angle of the steering wheel and the speed at which it is being turned. The signal is mainly used by the ABS System as part of it's stability control function but also by other systems such as ride level control and adaptive lighting. A problem with the SAS Signal will cause a fault with any of the systems that use the signal directly, or indirectly.
If the Steering Angle Sensor (SAS) needs to be changed, many vehicles require the new sensor to be calibrated. The iCarsoft VAWS V2.0 will allow you to carry out steering angle re-calibration on supported models.
ETCs Reset Function
Electronic Throttle Control system (ETC) relearns the throttle valve control value while clear or replace the throttle valve.
BMS Reset Function
Battery Management System (BMS), registers new battery to the BMS while battery replacement.
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Injector Programming
Injector coding, relearn the injector control parameter while the injector renewed or replaced

SPCIFICATIONS:
Display: 4.0″TFT LCD, 480*320 Pixels
Operation Temperature: 0°C ~ 50°C
Storage Temperature: -20°C ~ 70°C
Operating Voltage: 9 ~ 18V
Operating Current: 150mA@12V(Typical)
Power Consumption: 1.8W(Typical)
Dimension: 206*104.1*32.6 mm (L x W x H)

CONTENTS:
VAWS V2.0 Main Unit
Main Cable
USB Cable
TF Card
User Manual
Nylon carry case

VAWS V2.0 vehicle coverage of Audi/VW/Seat/Skoda:
(If your vehicles are before 2004 year, please make sure your vehicles are OBDII compliant firstly)
Audi:
A1               2011 - 2017
A2               2001 - 2006
A3               1997 - 2017
A4               1998 - 2017
A5               2008 - 2017
A6               1998 - 2017
A7               2011 - 2017
A8               1999 - 2017
Cabriolet          2003 - 2009
Q3               2012 - 2017
Q5               2009 - 2017
Q7               2007 - 2017
R8               2007 - 2017
TT               1999 - 2006

VW:
Amarok               2010 - 2015
Beetle                2012 - 2015
Beetle Cab            2013 -
Beetle Cab(NAR)       2012 -
New Beetle            1998 - 2011
New Beetle Cab         2003 - 2011
New Beetle Cab(NAR)   2010
New Beetle(NAR)       2010
Bora                  1995 - 2005
Bora(CHN)            2013 -
CaddY                2011 - 2015
CaddY                1996 - 2010
Corrado              1995
Crafter LT3            2006 - 2015
Eos                  2006 - 2007
Eos(NAR)             2010 -
Fox/CrossFox/Lupo     2004 - 2017
Gol Par Sav Poi        1999 - 2015
Gol Special            1999 - 2005
Gol/VoYage/Saveiro     2009 - 2013
Golf                  1998 - 2017
Golf Cabrio            1995 - 2002
Golf Cabriolet          2012 - 2017
Golf Jetta II             1995 - 2010
Golf Jetta VI            2009 - 2014
Golf Jetta VI(NAR)        2010 - 2014
Golf Plus               2005 - 2014
Golf Variant VII          2014 -
Golf Vento II           1995 - 1999
Golf/Jetta VII           2013 - 2017
Jetta                  2005 - 2010
Jetta IV                1999 - 2015
Jetta(CHN)             2013 -
Kombi                 2006 - 2015
LT2                   1996 - 2006
Lupo                  1999 - 2006
Novo Gol/VoYage/Saveiro 2013 - 2017
Passat                 2010 - 2017
Passat (B4,B5.B6.B7.CC)   1995-2017
Phaeton D1             2003 - 2017
Polo                   1995 - 2017
Polo Classic             1996 - 2010
Polo Vivo               2010 - 2015
Rabbit                 2006 - 2009
Sagitar                 2006 -
Santana                2001 - 2007
Sharan                 2001-2017
SpaceFox/SpaceCross/Suran/Sportva	 2006 - 2017
T4 Caravelle          2001 - 2003
Tiguan              2008 - 2017
Touareg             2003-2017
Touran              2003 - 2017
Transporter          1995-2015
Transporter/Multivan  2004-2015
Up                 2012 - 2017
XL1                2013 - 2017
Tiguan(NAR)         2010 -
Golf Variant VII       2014 -
Golf              2013 - 2015
Sagitar            2006 -
Touareg(NAR)      2011 -
Jetta(CHN)         2013 -
Bora(CHN)         2013 -

SEAT:
Alhambra I        2001 - 2010
Alhambra II        2011 - 2015
Altea             2004 - 2015
Arosa             2001 - 2004
Cordoba          1999 - 2009
Exeo             2009 - 2014
Ibiza             1999 - 2016
Inca              2001 - 2003
Leon             2000 - 2015
Mii               2012 - 2015
Toledo            1995 - 2010
Toledo            2013 - 2015

Skoda:
Citigo             2012 - 2017
Fabia              2000 - 2017
Felicia             1995 - 2001
Octavia            1997 - 2017
Rapid             2012 - 2017
Roomster          2006 - 2015
Superb            2002 - 2017
Yeti               2010 - 2017


